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NAME OF PARTS

MATERIAL

RESILIENT-SEATED GATE VALVE
AWWA C515 600PSI DN65-400

TEST PRESSURE

BODY

60

SEAT

44

WORKING PRESSURE

40

FLOW MEDIUM

SUITABLE TEMPERATURE





