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1 Q{ Working Pressure |10,/16 /25
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2 Media Available Water
{5 Bolt B.8(Calvanizing)
Bolt B.8(Calvanizing)
Bolt B.8(Calvanizing)
Cap/Handwheel Ductile iron
NBR Wi i
= ol m iper Ring NBR
5 5 8 Spindle Gland Ductile_iron
"o" Ring NBR
Gland Gasket NBR
) Back seat Gasket Nilon_1010
— 1 7 Bonnet Dustile iron
] Middle end seat _ring NBER
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2 Stem nut Brass
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S'pecification
Working Pressure 1.0/1.6
Test Body 1.5/2.4 MPa
Pressure| Soat 11,176
Working Temp. £66°C
Media Available Water
NBR Wiper Ring EPDM.
Eye bolt Carbon Steel
Bolt Carbon. Steel
Form_gear
Spindle Gland Ductile iron
Packing Crephite
Ciand Gasket WBR
FRoll bearing Carbon stesl
“o" Ring NBR
Bonnet Ductile iron
Boit Carbon Steel
Stem 85420
Stem nut Brass
Disc EPDM Coated D.1.
Body Ductile iron
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