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Nomina| "gptb-l6ce | BS4504-FNID | BS4504-FNIE | BS4504-PN25
size [T17pa) [1m6) 0 9 [ C Tn—od | oD [ oC [n-sd
DN50 | 150 [ 260 125 165 | 125 [ 4-19 | 165 125 [ 4-19
DN65_| 170 [270 145 165 | 145 | 4-19 | 165 | 145 | 6-19
DNE0_| 180 | 280 160 200 160 | 810 | 200| 160 | 8-10
DNIOO | 100 [ 300 180 720 180 [ 8-13 | 35| 190 [ 6-%0
DNi50 | 210 | 350 240 285 | 240 523 | 00| @50 628
DN200| 230 | 400 705 340 295 | 12-23 860 910 | 12-78
DN250| 250 [ 450 50 405 | 955 | 12—R6| 425 ] B70 | 1o-01
DN200| 270 | 500 200 450 410 | 12-28] 485| 430 [ 16-51
DN250 | 290 [ 550 750 520 | 470 16-28| 555 | 490 [ 16-04
DNZ00| 310 | 600 515 580 | 575 | 16-01 | 620 550 | 16-87
DNZ50| 330 | 650 565 640 585 | 20-31] 70| 600 | 20-57]
DN500 0 [ 700 520 715 | 850 | 20-34] 730 | 660 | 20-37]
DNE00| 390 [ 800 R €40 770 | 20-37] 845] 770 20-40)

WORKING PRESSURE 1.0/1.6/2.5
BODY |1.5/2.4/3.75 | MPa
TEST PRESSURE
SEAT |L1/1.76/2.75
WORKING TEMPERATURE 160°C
FLOW MEDIUM WATER
Cap/Handwheel Ductile Iron
Gland Brass
“o" Ring NBR
Bonnet Ductile Iron
Middle end seat ring EPDM
Stem 55420
Stem nut Ductile Iron
Gate EPDM Costed D.L
Body Ductile Iron
COMPONENT MATERIAL
DIN D.1 RESILEENT-SEAT
GATE VALVE DRAVD MARE [GUANTYTY| FIEY | sous
e T DN50-600
DRy ormous o vz pmemms
e o ASSEMBLY DRAVING
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Nominal| FoGgrEosface |  BS4504-PNIO BS4504-PNLE
SZ€ [ 4y [usssies| o0 [ 9C | n-0d | D [ #C [n-od
DN700 | 430 | 610 | B9S| 840 [24-3[] 210 | 840 24-37)
DNB00 | 470 | 660 |1015 | 950 | 24-34| 1025 950 | 24-40
DNI00 | 510 | 711 |15 | 1050 | 28-34| 1125 | 1050 | 28-40
DNI000| 550 | 813 |1230] 1160 | 29-37| 1255| 1170 | 28-43
DNIZ00 960 | 1455] 1390 32-40] 1485] 1390 32-49)
DNL400 1080 1675|1590 36-43| 1685 1550| 36-49
S'pecification
Working Pressure 1.0/1.6
Test Body 1.5/2.4 MPa
Pressure| Soat 11,176
Working Temp. £66°C
Media Available Water
NBR Wiper Ring EPDM.
Eye bolt Carbon Steel
Bolt Carbon. Steel
Form_gear
Spindle Gland Ductile iron
Packing Crephite
Ciand Gasket WBR
FRoll bearing Carbon stesl
“o" Ring NBR
Bonnet Ductile iron
Boit Carbon Steel
Stem 85420
Stem nut Brass
Disc EPDM Coated D.1.
Body Ductile iron
COMPONENT MATERIAL
RESILIENT-SEATED
GATE VALVE
DN700-1400





