闸阀

软密封闸阀（RESILIENT SEATED GATE VALVE）

Dimensions(mm)：DN40-DN1200
Working Pressure：Class 125/150

Valve Standard：EN1074-1 /2 AWWA C509/C515（WRAS证书、NSF检测报告、1074证书）
Face to Face：EN558-1 SERIES 3（B16.10）

Flange Type：ANSI B16.1/B16.5

Test standards：API598
Temperature：≤80℃

Thickness of anti-corrosion coating： ≥250UM.

执行器类型：手动 带标准操作齿轮箱.可配电动执行器和气动执行器.操作齿轮箱防护等 IP67(IP68可选)
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Working Pressure 16
Test Body 24 Bar
[Pressure[ Seqt 7.6
Working Temp. <B5°C
Media Available Water

Bore lb.8(catvanizing)

Bolt . 8(Calvanizing)

Botz . 8(Gulvanizing)

Cap /Handwheel Ductite sron.

NBR Wiper Ring NER

Spindie Gland Dustite_iron
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Gland Casket NBR

Back_seat Casket Niton 1010

Bonnat Dustile_iron
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COMPONENT MATERIAL

RESILIENT-SEATED
CATE VALVE gy e ey P
DN50-600 15018

[

0T

E ASSEMBLY DRAWING





[image: image2.jpg].

Nomlnol | Fece-to-face

Takle 9-Dimensians of IS0 flanges
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DN1200 960 1511 14225 | 44-41 70
DN1000 813 1289 | 1200 | 36-41 66
DN900 711 1168 | 1086 | 32-41 60
DN800 660 1060 | 978 28-41 60
DN700 610 927 | 864 28-35 54
Specification
Working Pressure 1.6

Test Body 2.4 MPa
Pressure| soqr 176

Working Temp. £65°C
Media Available Water

NBR Wiper Ring EPDM

Eye boit

Carbon_Steel

Boit

Carbon Steel

Worm gear

Spindle Gland Dustile_iron
Packing Graphite
Gland_Casket NBR
Roll._bearing Carbon steel
"o"_Ring NBR

Bonmet Dustile_iron
Bolt Carbon_Steel
Stem 55420
Stem_nad Brass

Diso EPDM Goated D.I.
Body Dustile_iron
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