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COMPONENT MATERIAL

MATERIAL LIST
Automoatic Air Valves (Double Ball)
DNS0-200

BODY |15/84/375
SEAT | 11/17.6/275| bar

WORKING PRESSURE 10/16/25

TEST PRESSURE

FLOW MEDIUM WATER
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