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SECTION
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NOMINAL | NOMINAL | SERVICE ALLOWED LENGTH THICKNESS  [HEIGHT| g oo
PIPE PIPE  [CONNECTION| TAPFING SIZE, |MM (MIN.) Mt MM
SIZE | OUTSIDE | SIZE IS0 7 THREAD ) T 172 ] H | NooF | BoTs
MM | DIA, MM MM DESIGNATION (4) (rRes) | MAX. BOLTS | SiZEw
50 63 55 3/t 700 5187 [ 3 T 76
75 o0 = 3/ 110 G U A 4 16
32 [ 5 (107 |35
55 3/t 5 108 [ 40
100 "o 32 1 120 5 10 8 40 4 16
50 1-1/2 5 [10]8 | 40
25 378 6 1128 | 40
150 180 32 [ 120 6 |12 8 [ 40 4 16
50 1-1/2 B 12 8 40
25 3/4 B 14 8 45
200 225 ER [ 120 6 | 148 | 45 4 16
50 1-1/2 6 | 148 | 45
25 374 7 |16 | & 50
32 1 120 7 16 8 50
a0 e 50 1-1/2 7 168 | 50 * *
63 2 40 7 |16 [ 8 | 50
25 374 7 18] 8 50
32 1 120 8 18 8 50
00 8 50 1-1/2 5 |18 ]8 | 50 * ®
63 2 40 8 |18 |8 | 50
PVC/PE PIPE

BOLTS & NUTS

D OF PIPE

T

LENGTH (L}

ELEVATION

)

PLAN

D.I. Saddle Clamp for PVC & PE Pipes

NOTES:

1. MATERIAL IS DUCTILE IRON CONFORM TQ ASTM A—536

2. MATERIAL OF BOLTS & NUTS IS STEEL CONFORM TO ASTM A-307
GRADE B, AND ASTM A-563 REPECTIVELY HOT DIP GALVANIZED
AS PER ASTM A—153.

3. SADDLE GLAMP SHOULD NOT LEAK OR BREAK WHEN TESTED WITH
TEST PRESSURE AT 2.0MPa FOR NOT LESS THAN 60 SECOND

4. COATING—BITUMINOUS COALTAR ENAMEL AT LEAST 50 MICRONS THICK

5. TAP THREAD AND DESIGNATION SHALL CONFORM TO IS0 7-Rc

6. RUBBER GASKET SHALL BE EPDM, SBR,NBR OR BUNA N IN ACCORDANCE
WITH IS0 4633 CLASS 70 & SUITABLE FOR DRINKING WATER.

7. PRIOR T DELIVERY AND ACCEPTANCE, SADDLE CLAMP SHALL BE TESTED
IN ACCORDANCE WITH MWSI SPECIFICATION WITNESSED BY MWS| REPRESENTATIVE.





