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COMPONENT MATERIAL
MATERIAL LIST
NO. | DATE | MODIFICATIONS | DESIGNED BY | VERIFIED BY | APPROVED

SINGLE SMALL ORIFICE(SSL)

TEST PRESSURE

BODY |15/24/37.5
SEAT |11/17.6/27.5] bar

WORKING PRESSURE 10/16/25
WORKING TEMPERATURE <60 °C
FLOW MEDIUM WATER

Model Drawing NO:

JIHIRY-18Q SSL




[image: image2.jpg]SIZE R
DN
15 |G1/2
20 |G 3/4
o5 |G U
32 |G 1-1/2
40 |G 1-3/4
50 |G 2

Bolt 55304

Small cover Ductile_iron

Air_release nuts | Brass

Plate Ductile_iron

Gasket NBE

Body Ductile_iron

Ball 55304

COMPONENT MATERIAL

MATERIAL LIST
NO. | DATE | MODIFICATIONS | DESIGNED BY | VERIFIED BY | APPROVED

SINGLE SMALL ORIFICE(SSL)

TEST PRESSURE

BODY |15/24/37.56
SEAT |11/17.68/27.5| bar

WORKING PRESSURE 10/16/25
WORKING TEMPERATURE <60 °C
FLOW MEDIUM WATER

Model Drawing NO:

JIHIRY-16Q SSL





