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Cover Ductile iron
Gosket NBR
Filter core S8304
Nut SS304
Bolt SS304
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Ductile iron filtrote valves

DNS0~600
TEST PRESSURE BODY |15/24/37.5
SEAT11/17.6/275| bar
WORKING PRESSURE 10/16/25
FLOW MEDIUM WATER





