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- Bolt Carbon steel
j Gasket WER
Bonnet Ductile Tron
NL Bolt Carbon steel
Y™ Filter screen 85304
Body Ductile iron
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TEST PRESSURE 5 loret
SEAT 11/17.6 | bar
WORKING PRESSURE 10/16
FLOW MEDIUM SEWAGE





