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Right body Dactile iron
Spannher Doctile iron
Packing glond | Dactile iron
Stem Stainless Steel
Packing PTFE
Ball SS304
Ad Just washer|PTFE
Left bod Dactile iron
COMPONENT MATERIAL

BALL VALVE

DN15~300

WORKING PRESSURE .0/1.6
BODY | 1.5/R.4 MPa

TEST PRESSURE

SEAT | 1.1/1.7
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g|Right body Ductile iron
7/Spanner Ductile iron
_ _ &|Packing gland Ductile iron
S|Stem SS420
4|Packing PTFE
! 3| Ball SS304
2| Ad just washer PTFE
LlLeft bod Ductile iron
Nol COMPONENT MATERIAL
SR ! BALL VALVE 150LB
E? DN50~200
l«
WORKING PRESSURE L6
BODY 2.4 MPa
TEST PRESSURE SEAT 178
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8|Right body Ductile iron
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_ _ _ &|Packing gland Ductile iron
5/ Stem SS420
4|/Packing PTEE
3/ Ball SS304
2| Ad just washer PTFE
LlLeft bod Ductile iron
Nd. COMPONENT MATERIAL
BB | BALL VALVE 10 kgf/cm
8 DN50~200
g
WORKING PRESSURE 1.0
BODY 2.1 MPa





