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DNISO 140
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Worn gear

shaft bearing

Stainless steel with PTEF lining

Stem

SS420

Pin

Carkon Steel

Disc

Ductile iron

Body seat ring

EPDM

Booly

Ductile iron

m

0-Ring

EPDM

Shoft end cover

Carbon Steel

Bolt

Stainless steel

COMPONENT

MATERTAL

MATERIAL LIST

BUTTERFLY VALVE

n-oy

TEST PRESSURE BODY 15/24

SEAT 11/176 Bar
WORKING PRESSURE 10/16
FLOW MEDIUM Pop—

SUITABLE TEMPERATURE

<650





