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Nominal| PSSt BS4504-PN10

BS4504-PN16

BS4504-PN25

4D

S1ze [ Fay [ICFie) | @D [ 9C [n-2d | 9D | 8C [ n-od | 9D [ @C | n-od
DNI00 | 190 | 127 | 220 200 |8-13 | 220 200 [8-19 | 235 190 [8-23
DNISO | 210 | 140 | @85] 240 8-23 | 285 240 8-23 | 300 | 250 |8-28
DNZ00 | 230 | 152 | 340 295 | 8-23 | 340 | 295|12-23| 360 | 310 |12-28
DN2S0| 250 | 165 | 395] 350 | 12-23| 405 | 395|12-28| 425 370 |12-31
TN300 | 270 | 176 | 445 400 | 12-23| 460 | 410 | 12-28 485 | 430 |16-31
DN350| 290 | 190 | 505 | 460 | 16-23| 520 | 470 | 16-28 553 | 490 |16-34
DN400 | 310 | 216 | 565 S5 | 16-28 | 580 | 525 16-31 | 620 | 550 | 16-37
TN450| 330 | 222 | 615 | 565 | 20-28| 640 | 585| 20-31 | 670 | 600 | 20-37
DNS00 | 390 | 229 | 670 | 620 | 20-28| 715 | 650 | 20-34| 730 | 660 | 20-37
DNe00 90 €7 | 780 | 725[ 20-31| 840 | 770 | 20-37 | 845[ 770 | 20-40
DN700 | 430 | 292 | 895 840 | 24-31| 510 | 840 | 24-37| 960 6/5|24-43
DNB00 [ 470 18 | 1015 | 950 [ 24-34| 1025 | 950 | 24-40 1085 [ 990 | 24-45
DN00 | 510 | 330 |15 | 1050 | 26-34| 1125 | 1050 | 28-40] 1185 | 1090 | 26-49
DNTO00| 550 | 410 [1230] 1160 | 28-37| [255] 1170 | 28-43[ 1320 (210 | 28-56
DNIZ00] 630 | 470 |1455| 1380] 32-40| 1485] 1390 32-49| 1530 1420| 32-56
DNL400] 710 | 530 | 1675[1590] 36-43] 1685 1590] 36-43]1755] 1640] 36-62
DNIEO00] 790 | 600 | 1915 [ 1820] 40-49] 1930 1820] 40-56 | 1975] 1860] 40-62
DNIS00[ 870 | 670 |2115[2020] 44-49[ 2130 2020] 44-56] 2195] 2070 44-70
DN2000 950 | 760 | 2325 2230] 48-49] 2345 2230 48-62] 2425 2300] 48-70

shaft bearing

Stainless steel

with PTEF lining

Shaft end cover

Ductile iron

Hondwheel

Ductile iron

Wormgear actuator

(for handwheel

operation)

Bolt Stainless steel
Disc Ductile iron
Stem Stainless steel

Disc seat ring cover| Stainless steel

N
==Y
gl A
4 b wsd
) !
o 27220\
g
= L

Disc seat ring EPDM
Seat of bod Stainless steel
Body Ductile iron
COMPONENT MATERIAL
BUTTERFLY VALVE

BODY B
WORKING PRESSURE 10/16/25
FLOwW MEDIUM WATER
SUITABLE TEMPERATURE <65°
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Slze b %D 90, | n-%d t | n-M
4” |DN100_| 127 [ 229 [1905 [8-19 24
67 [DN150 | 127 279 [2415 [8-22 26
g7 [DN200 [ 152 | 343 [2985[8-22 [28.6
10" |DN250 | 203 | 406 |362.0 |12-25|30.2
127[DN300 [ 203 | 483 [432.0 [12-25[31.8 ¥-7/8
127[DN350 | 203 | 933 [476 12-29] 35 [4-1"
16*|DN400 | 203 [ 597 [533.5[16-29[36.6 [4-1"
207|DNS00 | 203 [ 699 635 [20-32[42.5 1 1/
24/ DNG00 | 203 | 813 | 7495 |20-35 47,7 j1—1 1/4*
307|DN750 | 305 | 984 [914.4 [28-35] 54 p-1 1/4°
32/DNS00 | 305 | 1168 [1086 [32-41[60.4 4-1 172"
42| DN10S0| 305 | 1346[1257.5/36-41 | 66,7 41 1/2*
4g°|DN1200| 381 | 1511 [1422.5/44-41]69.9 4-1 1/2*

shaft kearing

Stalnless steel with PTEF Uning

Shaft end cover

Steel

Bolt

Galvanized steel

Hardwheel

Tuctlle Iran

Warngear actuator

Bolt

Stainless steel

Disc cover

Ductile iron

Sten

Stainless steel

Tisc

Tuctlle Iran

Disc_seat ring cover

Stainless steel

Disc_seat ring

EPDM

Seat of bady

Stalnless steel

Body

Tuctlle Iran

COMPONENT

MATERIAL

MATERIAL LIST

n-gd

BUTTERFLY VALVE AwWWwA C504 150LB
TEST PRESSURE PODY G
sear 76 Bar
WORKING PRESSURE i
FLOW MEDIM VATER
SUITABLE TEMPERATURE <=65°

Madel Draving NO





