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Working Pressure 16
Test Body 24 Bar
Pressure seqt 17.5
Working Temp. <65°C
Medio Availakle Water
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0-Rihg NBR
Nut carbon steel
gosket Carbon steel
shackles Carkon_steel
cover Ductlle Iran
gosket NER
0-Ring NER
0-Ring NER
Captop Tuctile Iron
Bolt carbon stee
Bonnet Tuctlle Tron
Stem Nuf Tuctile Iron
Stem 2cr1a
Disc Ductile Iron
Bod Ductlle Iran
COMPONENT MATERIAL





