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COMPONENT MATERIAL

MATERIAL LIST

Cost Iron Angle Valve
TEST® PRESSURE BODY [1.05/21/3.3
SEAT [0.77/1.54/2.48 wpa
WORKING PRESSURE 0.5/10/16
FLOW MEDIUM WATER
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