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Seat of body Stainless steel/Bronze
Seat of wedge Stainless steel/Bronze
] Bolt Carbon steel
Hexagon nut Carbon steel
needle Brass
71 nnn} direction Brass
L D Handwheel Cast iron
1 Spacer Carbon steel
Screw Carbon steel
a Packing gland Ductile iron
WA g A T Bolt o Carbon steel
Hexagon nut Carbon_steel
778@ Packing Expantion graphite
Gland box Cast iron
Gasket Graphite
=gl & Stem Stainless steel/Bronze
Bonnet Cast iron
Hexagon nut Carbon steel
Bolt Carbon steel
L washer Graphite
stem nut Bronze
\‘E Wedge Cast iron
L — Body Cast iron
JIS F 7363 JIS F 7364 TS F 7369 Eotpoent Material
DN L @D | ¢C |n—9d | L D | ®C |n—»d | L #D | ¢C |n—od Cast iron CGATE Valve
50 |180 130|105 | 4-15 | 200|155 |120 | 4-19 |200|155 120 |8-19
85 [190[155 [130 [ 4—15 220175 [140 | 4-19 [220[175 [140 [8-19 TEST PRESSURE | BODY |1.05/2.1/3.3
80 |200[180 [145 [ 4—19 |[230]185 [150 | 8-19 |230|200]160 |8—23 SEAT [0.77/1.54/2.42 | ypa
100 [230]200]165 | 8-19 | 250|210 |175 | 8-19 |250)225)|185 | 8-23
125 [250]235(200 | 819 |270| 250|210 | 8-25 | 270|270 225|8-25 WORKING PRESSURE  |0.5/1.0/1.6
150 |270]265[230|8-23 |290|280|240)|8-23 [290|305|260|12—-25 FLOW MEDIUM WATER
200 [280|320(280|12-23]320|330|290|12—-23|370| 350|305 |12-25 Model Drawing NO.
250 | 330| 385|345 (12-23| 380 | 400|355 |12—25|430 430|380 [12-27
300 |370[430]390[12-25|440 | 445 [ 400 [16—25]490 (480 |430[16-27





