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Pin Corbon steel

Nut Corkon steel

Spindle nut Corbon steel
Handwheel Cast iron

Packing Flexikle Graphite
Bonnet Cast Iron

Stem stainless steel/Bronze
Packing glond Brass

Seat ring Bross

Disc nut Bross

Disc stainless steel/Bronze
Valve seat stainless steel/Bronze
Body Cast Iron

COMPONENT MATERIAL

MATERIAL LIST

Cast Iron Gloke Valve
“ERT PUESSRE BODY [ 1.05/2.1/3.3
SEAT[0.77/154/2.42| wpo.
WORKING PRESSURE 05/1.0/L6
FLOW MEDIUM WATER
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