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Seat of body Stainless steel/Bronze
Seat of wedge Stainless steel/Bronze
I Bolt Carbon steel
Hexagon nut Carbon steel
needle Brass
[TIT1 [TTL direction Brass
4 N Handwheel Cast iron
N Spacer Carbon steel
Screw Carbon steel
‘ Packing gland Brass
A g % ‘ Bolt Carbon steel
Hexagon nut Carbon_steel
%7iw Packing Expantion graphite
Gland box Cast Steel
Gasket Graphite
zls| g Stem Stainless steel/Bronze
Bonnet Cast Steel
Hexagon nut Carbon steel
Bolt Carbon steel
L % washer Graphite
stem nut Bronze
\El Wedge Cast Steel
L — Body Cast Steel
TS T 7566 Component Material
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