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% : Pin Corbon steel
Nut Corbon steel
N Spindle nut Corbon steel
Handwheel Cast Steel
\ / Packing Flexible Graphite
Bonnet Cast Steel
N Stem stainless steel/Bronze
Packing gland stainless steel
( ) Seot ring Brass
5! S Disc_nut Brass
A A Disc stalnless steel/Bronze
NI Valve seat stalnless steel/Bronze
Body Coast Steel
COMPONENT MATERIAL
MATERIAL LIST
1= Cost Steel Globe Volve
3 TEST PRESSURE BODY | 505vEl
b SEAT|  077/154 | mpa
L WORKING PRESSURE 0.5/1.0
FLOW MEDIUM WATER
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