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Captop Grey cast iron

Grand Ductile cast iron

"o" Rin, NBR

Back seat Plastics

Bonnet Ductile cast iron

Gasket Rubber

Spindle Stainless steel

Spindle nuts Brass

Wedge disc D.I coating EPDM

Bod. Ductile cast iron

COMPONENT MATERIAL

D.LRESILIENT-SEAT GET VALVE
DN50-300
BODY | 15/24
TEST PRESSURE AT | 1778 b
WORKING PRESSURE 10/16
FLOW MEDIUM WATER

Model Drawing NO.





