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BONNET DUCTILE TRON
GUIDING STEM STAINLESS STEEL
SPRING S8304

DISC DUCTILE IRON

0— RING EPDM

BODY DUCTILE TRON
COMPONENT MATERIAL

Silent Check Valve

DN50—400
BODY | 15/24
TEST PRESSURE
SEAT | 11,/17.6 | bar
WORKING PRESSURE 10,16
FLOW MEDIUM WATER
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